
=================================
ASCII Configuration Command Hints
=================================

The bytes in the packets are continuous and contiguous when transmitted.
LabVIEW "textboxes" have a hexadecimal mode which provides an efficient
method of cutting and pasting byte data that would otherwise not be viewable.

As a rule:
1. When viewing packet byte data the textboxes are set to hexadecimal mode.
2. When viewing ASCII data (like ASCII configuration commands) the
        textboxes are set to normal character mode.
3. All ASCII configuration commands MUST be actual upper case ASCII characters.
4. Textbox characters in hexadecimal mode are automatically formatted with 
        spaces after each pair of bytes for display purposes only.
5. Bytes in hexadecimal display format can be cut/pasted between documents and
        hexadecimal mode textboxes.
6. ASCII configuration commands MUST be properly formatted to be accepted by
        a DPP device. (Ex. MCAC=1024 PRET=10  --> MCAC=1024;PRET=10;)

