# EthernetUtility.exe -

# Ethernet, Local System, and IP Address Configuration Utility

- Detects Local System:
  - Host Name
  - Host IP Address
- Perform NetFinder Search for connected Amptek Ethernet devices (LAN)
  - Searches and displays up to 4 devices
  - Select and test device found
  - Can send "Allow Sharing" Command to Amptek found device on Local Area Network
- Find Amptek Ethernet Device on Internet by "Type In IP Address" (WAN)
  - Internet connect uses point to point "Amptek Netfinder Packet"
- Perform IP Address Configuration for connected Amptek Ethernet devices (LAN)
  - Read Amptek Ethernet device IP Address Configuration
    - IP Address Type (Static or Dynamic)
    - IP Address
    - Subnet Mask
    - Gateway
    - MAC Address
  - Program Amptek Ethernet device IP Address Configuration
    - IP Address Type (Static or Dynamic)
    - IP Address
    - Subnet Mask
    - Gateway
  - Locked "Program IP Address Configuration" Send
  - To Program IP Address Configuration (LAN Only):
    - Select Device (use Select IP # button)
    - Find DPP IP (Found + IP Address will be displayed)
    - In the "DP5 IP Address Configuration" Group, press "Get from DP5"
    - The current IP Address configuration should be displayed
    - Set the new IP Address configuration
    - Press the "Unlock IP Configuration Send" button (Unlock Send)
    - In the "DP5 IP Address Configuration" Group, press "Send to DP5"
- "Copy to ClipBoard" creates DPP Ethernet Report
  - Press "Get Local System"
  - Select and Find a DPP Ethernet device
  - In the "DP5 IP Address Configuration" Group, press "Get from DP5"
  - Press "Copy to ClipBoard" to create DPP Ethernet Report
- Save and Restore current settings
- DPP Ethernet Utility Screenshot and Example Report (See Below)
- Installation setup program for systems without Visual Basic
- Visual Basic 5,6 source code.

# DPP Ethernet Utility Screenshot
# DPP Ethernet Utility Report
    ============================
    DPP Ethernet Utility
    ============================
    2/12/2013 10:09:30 AM

    ----------------------------
    DP5 IP Address Configuration
    ----------------------------
    Dynamic: Obtain IP address via DHCP
    IP Address 255.255.255.255
    Subnet Mask 255.255.255.255
    Gateway 255.255.255.255
    MAC Address 00-0C-9C-46-2A-43
    ----------------------------

    ----------------------------
    DPP Device Search Summary
    ----------------------------
    IP Address 192.168.0.226 Port 10001
    Found DPP at IP Address 192.168.0.226
    ----------------------------
    DPP Device 1
    Amptek DP5 - S/N 51110
    Connection: Interface is open (unconnected)
    IP Address: 192.168.0.226
    Amptek X-123 51110
    MAC Address: 00-0C-9C-46-2A-43
    Time Powered:  54 minutes,40 seconds
    Time on Network:  54 minutes,33 seconds
    ----------------------------
    ----------------------------
    DPP Device 2
    Amptek DP5 - S/N 19472
    Connection: Interface is open (unconnected)
    IP Address: 192.168.0.248
    XRF1 X123SDD (updated 8/10/10)
    MAC Address: 00-0C-9C-45-9D-33
    Time Powered:  25 days,0 hours,50 minutes,54 seconds
    Time on Network:  25 days,0 hours,50 minutes,52 seconds
    ----------------------------

    ----------------------------
    Local System
    ----------------------------
    Host Name       XRF_Worstation
    Host IP Address 192.168.0.219
    ----------------------------