	Multiple USB DPP README 20070613

NOTE: SEE AssignAppToDpp.pdf and SelectDpp.pdf


0.) This is an ADVANCED FEATURE, PLEASE read all the
    documentation.

1.) When enabled, ADMCA can be assigned to a DPP device.
      (AssignAppToDpp.pdf)

2.) ADMCA can read all USB DPP devices.

3.) If more than one USB DPP device is connected, devices can be selected from a list.
      (SelectDpp.pdf)

NOTE: YOU MUST SELECT THE CORRECT DEVICE TYPE BEFORE SELECTING A DEVICE
      FROM THE LIST OF AVAILABLE DEVICES.

4.) In AssignAppToDpp.pdf, UNIQUE unit number examples
      UnitNumber=Unit1
          OR
      UnitNumber=Office203

      ;Assign a UNIQUE unit number to your application.
      ;UnitNumber=YourUnitNumber


ADMCA Analog and Digital Acquisition Software (MCA8000A/DP4/X123/GAMMA-RAD/PX4)                 RNREV20070613
Copyright (C) 2005-2007 Amptek, Inc.

